[BAND NAME]  TECH SPEC
Version 1.0  ·  [DATE]  ·  On-the-night contact: [NAME] [PHONE]
Template by Seismic DSP · seismicdsp.com/guides/tech-specs. Replace everything in [brackets], delete anything that doesn't apply (it's deliberately complete), and delete all red text like this before sending.
About the Band
[Big Doinks is a four-piece guitar focussed down-tempo doom band. Drums (SPD pad running 2 backing tracks), bass (amp on stage), 2 guitars DI'd from pedalboards, and lead vocals, with backing vocals from guitar and bass.]
Contacts
	ROLE
	NAME
	PHONE
	EMAIL

	On-the-night contact
	[NAME]
	[PHONE]
	[EMAIL]

	Manager
	[NAME]
	[PHONE]
	[EMAIL]

	Technical
	[NAME]
	[PHONE]
	[EMAIL]


Stage Plot
	[Draw or paste your stage plot here. Simple shapes and labels: player positions, amps, pedalboards, racks, vocal mic positions, where you hand tails to the venue, and power drops with socket counts.]


Kit List
	GUITAR
	BASS
	DRUMS

	Pedalboard (DI x 2)
	Pedalboard (DI)
	5 piece drum kit + SPD (tracks)

	[Amp / cab if used]
	[Amp / cab if used]
	[Breakables needed from venue]

	Power: 2x 240V, DSR
	Power: 2x 240V, DSL
	Power: 3x 240V, USC




Monitors
[We carry our own IEM rack and mixer. We hand you tails from our analog splits.]
[We need one mono drum mix back from FOH on one XLR.]
[We'd like one wedge each side of the stage with a general band mix, no click.]
[We need N monitor mixes from the house console: ...]
Click is NOT routed to the main mix under any circumstances.
	MIX
	UNIT
	PURPOSE
	BAND
	FREQUENCY
	NOTES

	Mix 1
	IEM TX 1
	Band mix (guitar + bass packs)
	823-832MHz
	823.400 MHz
	Licence-free UK/EU

	Mix 2
	IEM TX 2
	Vox mix
	823-832MHz
	826.300 MHz
	Licence-free UK/EU

	Mix 3
	Drum pack
	Drum mix
	Wired
	—
	No RF

	[Mix 4]
	[Unit]
	[Purpose]
	[Band]
	[Frequency]
	[Notes]


Every transmitter you bring, with its exact frequency. Update whenever anything changes; check band legality for every country you play.
Tech Rider
This section scales with the show. At club level, delete most or all of it.
[PA: full-range system capable of 120dBA, clean and undistorted, at the mix position. Subs required.]
[We bring our own FOH engineer. House console is fine: current-generation digital preferred.]
[We bring our own monitor engineer and console at side-stage; we need power and space for it.]
[We bring our own vocal mics; everything else per the input list.]
[Side-stage: one table for the playback rig, 2x 240V, and space for a guitar tech.]
Notes for the Engineer
Guidance, not requirements: how to mix us to OUR taste. FX first, balance second.
[Lead vocal: long dotted-8th delay, big dark hall reverb.]
[Backing vocals: short plate reverb, texture behind the lead, not a second lead.]
[Guitars/synths: FX come off our rig, nothing needed at FOH. Synths sit under the guitars.]
[Drums: big and crushed, kick and snare forward.]
[Screams should cut; clean vocals can sit back.]
Before You Send This
☐  Deleted everything that doesn't apply (including all red text)
☐  Date and version updated, date in the filename
☐  One on-the-night contact named with a working phone number
☐  Stage plot matches the input list and kit list; RF table matches the rack
☐  Two printed copies on you at all times; assume the engineer has never seen your email


Input List
	CH
	SOURCE
	MIC / DI
	LOC
	NOTES

	1
	Kick In
	Beta 91
	USC
	

	2
	Kick Out
	Audix D6
	USC
	

	3
	Snare Top
	Audix i5
	USC
	

	4
	Snare Bottom
	SM57
	USC
	

	5
	Hi-hat
	sE Electronics SE8
	USC
	+48V

	6
	Rack Tom
	Sennheiser e904
	USC
	

	7
	Floor Tom
	Sennheiser e904
	USC
	

	8
	Spare
	
	
	

	9
	Overhead L
	sE Electronics SE8
	USC
	+48V

	10
	Overhead R
	sE Electronics SE8
	USC
	+48V

	11
	Bass DI
	DI Box
	DSL
	

	12
	Bass Mic
	Audix D6
	CS
	

	13
	Guitar 1
	DI (Quad Cortex)
	DSR
	

	14
	Guitar 2
	DI (Kemper)
	DSR
	

	15
	BV 1
	Sennheiser e945
	DSR
	

	16
	Vox
	Sennheiser e945
	DSC
	Supplied by artist

	17
	Vox Spare
	Sennheiser e945
	DSC
	

	18
	BV 2
	Sennheiser e945
	DSL
	

	19
	Track 1 (Guitars)
	DI Box
	USC
	

	20
	Track 2 (Synth/Vox/FX)
	DI Box
	USC
	

	21
	Track 3 (Sub Bass)
	DI Box
	USC
	

	22
	Click
	DI Box
	USC
	NOT ROUTED TO MAIN MIX.

	23
	Drums Shout
	Switched SM58
	USC
	NOT ROUTED TO MAIN MIX. Supplied by crew

	24
	Sidestage Shout
	Switched SM58
	SR
	NOT ROUTED TO MAIN MIX. Supplied by crew


* Mics listed are a preference. Where the listed make/model is unavailable, an industry-standard equivalent is acceptable.




